INPUT BEGIN
NEW EQUIPMENT /LCS2
POS W 6000mm N 10020mm U 1301mm
ORI Y is E and Z is U
BUIL false
DSCO unset
PTSP unset
INSC unset

NEW SUBEQUIPMENT
POS E 20mm N 30mm D 1326mm
BUIL false
DSCO unset
PTSP unset
INSC unset

NEW CYLINDER
POS W 100.5mm S 50mm U 1126.5mm
ORI Y is N and Z is D
DIAM 30mm
HEIG 15mm

END
NEW CONE
POS W 100.5mm S 50mm U 1119mm
DTOP 30mm
DBOT 25mm
HEIG 5mm

END
NEW CYLINDER
POS W 100.5mm S 50mm U 1145mm
DIAM 30mm
HEIG 10mm

END
NEW CYLINDER
POS W 100.5mm S 50mm U 1137mm
DIAM 25mm
HEIG 6mm

END
END
NEW SUBEQUIPMENT
POS E 20mm N 70mm D 1326mm
BUIL false
DSCO unset
PTSP unset
INSC unset

NEW CYLINDER
POS W 100.5mm S 50mm U 1126.5mm
ORI Y is N and Z is D
DIAM 30mm
HEIG 15mm

END
NEW CONE
POS W 100.5mm S 50mm U 1119mm
DTOP 30mm
DBOT 25mm
HEIG 5mm

END
NEW CYLINDER
POS W 100.5mm S 50mm U 1145mm
DIAM 30mm
HEIG 10mm

END
NEW CYLINDER
POS W 100.5mm S 50mm U 1137mm
DIAM 25mm
HEIG 6mm

END
END
NEW BOX
POS W 80.5mm N 0mm U 0mm
ORI Y is W and Z is U
XLEN 234mm
YLEN 161mm
ZLEN 352mm

END
NEW BOX
POS E 5mm N 0mm U 55mm
ORI Y is E and Z is U
XLEN 150mm
YLEN 10mm
ZLEN 50mm

END
END
INPUT END  EQUIPMENT /LCS2
INPUT FINISH
