INPUT BEGIN
NEW EQUIPMENT /吸顶防爆灯
POS E 115mm N 0mm D 115mm
ORI Y is N and Z is W
BUIL false
DSCO unset
PTSP unset
INSC unset

NEW CYLINDER
POS E 250mm N 0mm U 0mm
ORI Y is E 30 D and Z is N
DIAM 80mm
HEIG 30mm

END
NEW CYLINDER
POS E 165mm N 0mm U 0mm
ORI Y is N and Z is W
DIAM 20mm
HEIG 100mm

END
NEW DISH
POS W 10mm N 0mm U 0mm
ORI Y is N and Z is W
DIAM 150mm
HEIG 80mm
RADI 100mm

END
NEW CYLINDER
POS E 5mm N 0mm U 0mm
ORI Y is N and Z is E
DIAM 170mm
HEIG 30mm

END
NEW CYLINDER
POS E 50mm N 0mm U 0mm
ORI Y is N and Z is E
DIAM 130mm
HEIG 60mm

END
NEW CONE
POS E 97.5mm N 0mm U 0mm
ORI Y is N and Z is E
DTOP 20mm
DBOT 130mm
HEIG 35mm

END
END
INPUT END  EQUIPMENT /吸顶防爆灯
INPUT FINISH
