INPUT BEGIN
NEW EQUIPMENT /操作柱
BUIL false
DSCO unset
PTSP unset
INSC unset

NEW SUBEQUIPMENT /Copy-(6)-of-柱体
BUIL false
DSCO unset
PTSP unset
INSC unset

NEW CYLINDER
POS W 90mm S 90mm U 15mm
DIAM 12mm
HEIG 20mm

END
NEW CYLINDER
POS W 90mm N 90mm U 15mm
ORI Y is S and Z is U
DIAM 12mm
HEIG 20mm

END
NEW CYLINDER
POS E 90mm S 90mm U 15mm
DIAM 12mm
HEIG 20mm

END
NEW CYLINDER
POS E 90mm N 90mm U 15mm
ORI Y is S and Z is U
DIAM 12mm
HEIG 20mm

END
NEW CYLINDER
POS W 90mm S 90mm U 10mm
DIAM 24mm
HEIG 10mm

END
NEW CYLINDER
POS W 90mm N 90mm U 10mm
ORI Y is S and Z is U
DIAM 24mm
HEIG 10mm

END
NEW CYLINDER
POS E 90mm S 90mm U 10mm
DIAM 24mm
HEIG 10mm

END
NEW CYLINDER
POS E 90mm N 90mm U 10mm
ORI Y is S and Z is U
DIAM 24mm
HEIG 10mm

END
NEW BOX
XLEN 240mm
YLEN 240mm
ZLEN 10mm

END
NEW BOX
POS E 0mm N 0mm U 1005mm
XLEN 120mm
YLEN 60mm
ZLEN 2000mm

END
END
NEW SUBEQUIPMENT /Copy-(6)-of-控制盒
BUIL false
DSCO unset
PTSP unset
INSC unset

NEW BOX
POS E 0mm S 165mm U 1460mm
XLEN 80mm
YLEN 10mm
ZLEN 80mm

END
NEW BOX
POS E 0mm S 185mm U 1460mm
ORI Y is N and Z is W 45 U
XLEN 5mm
YLEN 20mm
ZLEN 50mm

END
NEW CONE
POS E 0mm S 171.5mm U 1550mm
ORI Y is U and Z is S
DTOP 25mm
DBOT 30mm
HEIG 3mm

END
NEW CYLINDER
POS W 40mm S 165mm U 1550mm
ORI Y is U and Z is S
DIAM 30mm
HEIG 10mm

END
NEW CYLINDER
POS E 0mm S 110mm U 1375mm
ORI Y is S and Z is D
DIAM 30mm
HEIG 50mm

END
NEW CYLINDER
POS E 40mm S 165mm U 1550mm
ORI Y is U and Z is S
DIAM 30mm
HEIG 10mm

END
NEW CONE
POS W 40mm S 171.5mm U 1550mm
ORI Y is U and Z is S
DTOP 25mm
DBOT 30mm
HEIG 3mm

END
NEW CONE
POS E 40mm S 171.5mm U 1550mm
ORI Y is U and Z is S
DTOP 25mm
DBOT 30mm
HEIG 3mm

END
NEW CYLINDER
POS E 0mm S 165mm U 1550mm
ORI Y is U and Z is S
DIAM 30mm
HEIG 10mm

END
NEW CYLINDER
POS E 0mm S 172.5mm U 1460mm
ORI Y is U and Z is S
DIAM 50mm
HEIG 5mm

END
NEW BOX
POS E 0mm S 110mm U 1500mm
XLEN 160mm
YLEN 100mm
ZLEN 200mm

END
NEW BOX
POS E 0mm S 57.5mm U 1500mm
XLEN 120mm
YLEN 5mm
ZLEN 210mm

END
NEW BOX
POS E 0mm S 45mm U 1607.5mm
XLEN 120mm
YLEN 30mm
ZLEN 5mm

END
NEW BOX
POS E 0mm S 45mm U 1392.5mm
ORI Y is N and Z is D
XLEN 120mm
YLEN 30mm
ZLEN 5mm

END
END
END
INPUT END  EQUIPMENT /操作柱
INPUT FINISH
