INPUT BEGIN
NEW EQUIPMENT /防爆手动报警按钮
POS E 859255mm N 1633800mm U 1300mm
ORI Y is W and Z is U
BUIL false
DSCO unset
PTSP unset
INSC unset

NEW CYLINDER
POS W 10mm N 35mm D 60mm
DIAM 10mm
HEIG 20mm

END
NEW CYLINDER
POS E 9.999mm N 35mm D 60mm
DIAM 10mm
HEIG 20mm

END
NEW DISH
POS W 35mm S 15mm U 0mm
ORI Y is U and Z is S
DIAM 20mm
HEIG 5mm
RADI 7.5mm

NEW NCYLINDER
POS E 0mm N 12mm U 0mm
DIAM 10mm
HEIG 10mm
PRODHT 'Hole'

END
NEW NCYLINDER
POS E 10.392mm N 6mm U 0mm
ORI Y is E 30 N and Z is U
DIAM 10mm
HEIG 10mm
PRODHT 'Hole'

END
NEW NCYLINDER
POS E 10.392mm S 6mm U 0mm
ORI Y is E 30 S and Z is U
DIAM 10mm
HEIG 10mm
PRODHT 'Hole'

END
NEW NCYLINDER
POS W 0.001mm S 12mm U 0mm
ORI Y is S and Z is U
DIAM 10mm
HEIG 10mm
PRODHT 'Hole'

END
NEW NCYLINDER
POS W 10.393mm S 6mm U 0mm
ORI Y is W 30 S and Z is U
DIAM 10mm
HEIG 10mm
PRODHT 'Hole'

END
NEW NCYLINDER
POS W 10.392mm N 6mm U 0mm
ORI Y is W 30 N and Z is U
DIAM 10mm
HEIG 10mm
PRODHT 'Hole'

END
END
NEW CYLINDER
POS W 35mm S 10mm U 0mm
ORI Y is U and Z is S
DIAM 5mm
HEIG 10mm

END
NEW CTORUS
POS E 5mm S 5mm U 0mm
ORI Y is U and Z is S
RINS 17mm
ROUT 25mm
ANGL 180degree

END
NEW CTORUS
POS E 5mm S 5mm U 0mm
ORI Y is D and Z is N
RINS 17mm
ROUT 25mm
ANGL 180degree

END
NEW BOX
XLEN 100mm
YLEN 10mm
ZLEN 100mm

END
NEW BOX
POS E 0mm N 35mm U 0mm
XLEN 100mm
YLEN 40mm
ZLEN 100mm

END
NEW BOX
POS E 0mm N 10mm U 0mm
XLEN 80mm
YLEN 10mm
ZLEN 80mm

END
END
INPUT END  EQUIPMENT /防爆手动报警按钮
INPUT FINISH
